GROW GREEN CONSTRUCTIONS

FOR HEALTHYCITIES

**9008855501**

**9611745906**

[**www.growgreenconstructions.com**](http://www.growgreenconstructions.com/) **email :** [**anil@growgreenconstructions.com**](mailto:anil@growgreenconstructions.com)



# Opp. Rural Police Station D.R ground, Chamundeshwari Nagar, Bannur Main Road, Mandya - 571 401

**Materials Detail For 1,75,000 Rs**

# Clint Name : Date :

**Ph.No = Place : Mandya**

1. Wire cut Bricks = 8.0Rs/Each
2. Ultratech Cement = 450 Rs/Bag 3] Turbo TMT Or = 66 Rs/kg
3. Sand = M –Sand For Concreeting & Brick Work, River Sand & P-Sand For Plastering.
4. Size Stone For 4 Sides Boundary (5 Course) = Nagamangala 6] Plumbing Pipes = Ashirvaad

7] Fittings & Sanitary = Cera 8] Wire = Finolex

1. Switches = Lisha Switches with metal box
2. Flooring Tiles = Vetrified (2x2) = 40 Rs Sqft 11] Elevation Tiles = 40 Rs

12]Parking Tiles = 28 Rs 13] Bath Room Tiles = 26 Rs

14] Pooja & Kitchen Tiles = 30 Rs 15]Commodes = 3,000 Rs (Floor Mounted) 16] Wash Basin = 1,000Rs

17]Taps = 250 Rs

18] Diverters With Spouts ( Ashirvaad )= 4,000 Rs 19] Kitchen Sink = 1200 Rs

20] Over Head Tank = 1000 ltr [3 Layer] 21]Main Door = Malesian Honne = 6”X4” 22]Pooja Door = Malesian Honne = 5” X 3”

23] Windows and Other Doors Frames = Neem Wood (5” X 3”) (Powder Coated Fittings) 24]Windows Shutters = Ulchi or Hercules (Powder Coated Fittings )

1. Flush Doors = 3000 Rs/ Door
2. Main Door Locks = 3,000 Rs (Europa) 27]Rooms & Bath Locks = Europa
3. Asian Paint = Inside 3 Coat Birla Wall Care With 2 Coats Of Premium Paint Outside 1 Coat of Primer & 1 Coat Of Apex Paint
4. Entrance Gate , Water Tank , Ladder & Stair Case = M.S Pipes With 14 Gauge thickness Railing